{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Experiment Metadata","G-85 A2","xhatch"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Experiment Metadata","index":0,"n_rows":47,"n_cols":23,"rows_kept":47,"cut":false,"hidden":false,"merged":[[31,3,31,4],[31,9,31,11],[19,2,19,3],[19,4,19,6],[19,9,19,10],[25,3,25,4],[26,3,26,4],[27,3,27,4],[28,3,28,4],[29,3,29,4],[25,9,25,11],[30,3,30,4],[30,9,30,11],[28,9,28,11],[29,9,29,11],[37,14,38,14],[37,10,37,13],[6,0,6,1],[1,0,1,1],[7,3,7,4],[8,3,8,4],[15,0,15,1],[16,9,16,10],[20,9,20,10],[17,9,17,10],[16,2,16,3],[17,2,17,3],[20,2,20,3],[16,4,16,6],[17,4,17,6],[20,4,20,6],[42,10,42,11],[44,10,44,11],[32,3,32,4],[38,10,38,11],[39,10,39,11],[40,10,40,11],[37,6,37,9],[32,9,32,11],[41,10,41,11],[43,10,43,11],[8,7,8,11],[2,2,2,11],[4,2,4,11],[7,7,7,11],[27,9,27,11],[3,2,3,11],[10,7,10,11],[11,3,11,4],[11,7,11,11],[26,9,26,11],[9,3,9,4],[9,7,9,11],[18,2,18,3],[18,4,18,6],[18,9,18,10],[10,3,10,4]]}
[]
["EXPERIMENT:"]
[null,"Title *","Pretreatment for benchmarking series 42"]
[null,"Description *","The purpose of this matrix was to evaluate different pretreatments on Quaker lubricated EForm Plus and as-received Eform Plus for corrosion protection properties."]
[null,"Methods *","Corrosion testing and cross-hatch adhesion testing (dry and wet) were completed in this experiment. Corroded panels were scraped to remove the built up corrosion product and the delaminated electrocoat, then the scribe creep was measured using calipers."]
[]
["CONTRIBUTORS:"]
[null,"Last Name *","First Name *","Email Address *",null,"Institution *","Phone Number","Mailing Address"]
[null,"Valdez","Lyanne","lvaldez@ppg.com",null,"PPG",null,"4325 Rosanna Drive, Allison Park, PA 15201"]
[]
[]
[]
[]
[null,"+Add Row"]
[]
["SOURCE MATERIAL:"]
[null,"Name *","Supplier/Provider *",null,"Description *",null,null,"Date Received *","Material *","Condition",null,"Location"]
[]
[]
[]
[]
[]
[null,"+Add Row"]
[]
["SPECIMENS:"]
[null,"Name *","Source Material","Processing *",null,"Creation Date","Thickness *","Width *","Area *","Comments"]
[null,null,"Name *",null,null,null,"mm","mm","mm^2"]
[]
[]
[]
[]
[]
[]
[]
[null,"+Add Row"]
[]
["TESTS:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TEST PARAMETERS",null,null,null,null,null,null,"+Add Column"]
[null,"Name *","Specimen Name *","Type of Test *","Operator *","Test Date *","Instrument",null,null,null,"Notes",null,null,null,"Files\n(supplemental data files associated with each test)","Property Name","Property Name","Property Name","Property Name","Property Name","Property Name","Property Name"]
[null,null,null,null,null,null,"Name *","Type *","Location *","Last Calibration Date *","Test",null,"Specimen","Instrument",null,"units","units","units","units","units","units","units"]
[null,"G-85 A2 testing"]
[null,"cross-hatch adhesion testing"]
[]
[]
[]
[]
[]
[null,"+Add Row"]

{"sheet":"G-85 A2","index":1,"n_rows":38,"n_cols":14,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,1,0,6]]}
["Test *","G-85 A2 testing Quaker lubricated and bare EFP 3/6 weeks"]
[]
["SUMMARY"]
[null,"Field Name: * ","Henkel/Quaker - C2.4 (6 weeks)","Henkel/Quaker - C2.4 + PT8 (6 weeks)","Xtalic/Quaker - C2.4 (3 weeks)","Xtalic/Quaker - C2.4 + PT8 (3 weeks)","Bare EFP - C2.4 (6 weeks)","Bare EFP - C2.4 + PT8 (6 weeks)","+Add Column"]
[null,"Units: * ","mm","mm","mm","mm","mm","mm"]
[null,"Scribe creep measurements",2.4550000000000001,2.3339999999999996,11.837,12.0715,1.6859999999999999,1.5339999999999998]
[]
[]
[]
[null,null,"Enter data here"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"+Add Row"]
[]
["TEST DATA"]
[null,null,"RAW",null,null,null,null,"+Add Column","CALCULATED",null,null,null,null,"+Add Column"]
[null,"Field Name: *","Property Name","Property Name","Property Name","Property Name","Property Name",null,"Property Name","Property Name","Property Name","Property Name","Property Name"]
[null,"Units: *","units","units","units","units","units",null,"units","units","units","units","units"]
[null,"Description: *","description","description","description","description","description",null,"description","description","description","description","description"]
[null,"Valid Min:"]
[null,"Valid Max:"]
[null,"Missing Value:"]
[null,null,"Enter data here"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"+Add Row"]

{"sheet":"xhatch","index":2,"n_rows":38,"n_cols":14,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,1,0,6]]}
["Test *","cross-hatch adhesion testing Quaker lubricated and bare EFP"]
[]
["SUMMARY"]
[null,"Field Name: * ","Henkel/Quaker - C2.4","Henkel/Quaker - C2.4 + PT8","Xtalic/Quaker - C2.4","Xtalic/Quaker - C2.4 + PT8","Bare EFP - C2.4","Bare EFP - C2.4 + PT8","+Add Column"]
[null,"Units: * ","N/A","N/A","N/A","N/A","N/A","N/A"]
[null,"dry",9,8.5,9,8,9,9]
[null,"wet",8.5,8,8.5,7.5,8,4]
[]
[]
[null,null,"Enter data here"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"+Add Row"]
[]
["TEST DATA"]
[null,null,"RAW",null,null,null,null,"+Add Column","CALCULATED",null,null,null,null,"+Add Column"]
[null,"Field Name: *","Property Name","Property Name","Property Name","Property Name","Property Name",null,"Property Name","Property Name","Property Name","Property Name","Property Name"]
[null,"Units: *","units","units","units","units","units",null,"units","units","units","units","units"]
[null,"Description: *","description","description","description","description","description",null,"description","description","description","description","description"]
[null,"Valid Min:"]
[null,"Valid Max:"]
[null,"Missing Value:"]
[null,null,"Enter data here"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"+Add Row"]